f/D = 0.4 Illumination taper = 10 dB

Figure 1. Typical vs. Desired Dish Illumination

N1BWT 1994

0 dB -10 dB -20 dB

Spillover loss

Illumination loss