Dish patterns with feed displaced axially from focus, by P.O. Figure 26

Dish diameter = 20 λ, f/D = 0.5 Feed diameter = 1.2 λ, Phase Center at feed aperture

a: Feed 2.0 wavelengths toward dish

E-plane

H-plane

0 -10 -20 -30

+10

+20

+30 dBi

b: Feed 2.0 wavelengths away from dish

E-plane

H-plane

0 -10 -20 -30

+10

+20

+30 dBi

c: Feed 3.0 wavelengths toward dish

E-plane

H-plane

0 -10 -20 -30

+10

+20

+30 dBi

d: Feed 3.0 wavelengths away from dish

E-plane

H-plane

0 -10 -20 -30

+10

+20

+30 dBi

W1GHZ 1998